*) HIGH-PERFORMANCE 2-WAY POINT-SOURCE ACTIVE SPEAKER

1. 개요

본 기기는 앰프내장형 2-WAY 포인트소스 스피커로 다음과 같은 규격에 준한다.

2. 기능 및 특성

130 dB SPL Max

Rotatable 100° x 50° TRW Horn

10" neodymium woofer, 2.5" voice coil

1,75" PKX dome, neodymium compression driver

2 channel, 2000 W Class D Amplifier

DSP Processing with FiRPHASE and BMC

RDNet Networked Management

powerCON TRUE1 TOP mains connectors

3. 규격 및 사양

Acoustical specifications

Frequency Response	: 60 Hz ~ 20000 Hz

Max SPL @ 1m	: 130 dB

Horizontal coverage angle	: 100°

Vertical coverage angle	: 50°

Transducers

Compression Driver	: 1 x 1.0" neo, 1.75" v.c

Woofer	: 10" neo, 2.5" v.c

Input/Output section

Input signal	: bal/unbal

Input connectors	: XLR, RDNet Ethercon

Output connectors	: XLR, RDNet Ethercon

Input sensitivity	: -2 dBu/+4 dBu

Processor section

Crossover Frequencies	: 1600Hz

Protections	: Thermal, HF

Limiter	: Fast Limiter

Controls	: Bypass, Linear/High Pass, Volume

RDNet	: Onboard

Power section

Total Power	: 2000 W Peak

High frequencies	: 600 W Peak

Mid frequencies	: 1400 W Peak

Cooling	: Convection

Connections	: Powercon TRUE1 TOP IN/OUT

Standard compliance

Safety agency	: CE compliant

Physical specifications

Cabinet/Case Material	: Baltic birch plywood

Hardware	: 3X M10 TOP AND BOTTOM,	2X PIN D.10 AND M10 SIDE

Handles	: 1 TOP

Pole mount/Cap	: 35 mm insert

Grille	: Steel with clothing

Color	: Black

Size

Height	: 510 mm / 20.08 inches

Width	: 300 mm / 11.81 inches

Depth	: 300 mm / 11.81 inches

Weight	: 14 kg / 30.86 lbs

* KX 10-A 동급이상품